**Preferred Method of Construction**

**At**

**1, 3 and 5 Park Street**

**Hatfield AL9 5AX**

**For**

**Hog Group - RWA Ref: RMW/11622/18**

**STAIRCASE PROPPING**

The existing staircase is propped but not adequately or undertaken in a permanent manner therefore to be supplemented by steelwork.

1. Leave all existing timber props in place and do not take out, alter, mend.
2. Insert 152x90 PFC steel channel or 152 UC into the existing side wall bearing onto engineering brick or concrete padstone to be fixed to the top of the longitudinal steel using a Lindaptor comnnector.
3. Provide shins or packing up to the underside of the existing soleplate to the affected lathe and plaster stud walling which carries the weight of the staircase winder. Packing not be over tightened but to work in tandem with the existing timber.