**Materials to be used in the construction of the external surfaces of the buildings**

**Stable Block**

**Roofing Materials**

* Natural roofing slates (matt finish) including all associated lead soakers, flashings hips, valleys etc…
* Plain painted timber fascia

**New External Brickwork**

* Soft red facing bricks to match existing

**Windows**

* Jeld-wen timber Elegance flush casement window – plain style – with curved timber filler piece to match existing

**External Doors**

* Jeld-wen Burlghley to match existing

**French Doors**

* Jeld – Wen Dreamvu

**Bi-Fold Doors**

* Smart Systems Visofold

 